
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "USB4085-GF-A_REVA4" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -5.08 18.288 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "USB4085-GF-A_REVA4" (id 1) (at -5.08 -20.32 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "GCT_USB4085-GF-A_REVA4" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "A4" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Global Connector Technology" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SNAPEDA_PN" "USB4085-GF-A" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARDD" "Manufacturer Recommendations" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.46 mm" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "USB4085-GF-A_REVA4_0_0"
      (rectangle (start -5.08 -17.78) (end 5.08 17.78)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin power_in line (at -10.16 15.24 0) (length 5.08)
        (name "VBUS"
          (effects (font (size 1.016 1.016)))
        )
        (number "A4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -10.16 15.24 0) (length 5.08)
        (name "VBUS"
          (effects (font (size 1.016 1.016)))
        )
        (number "A9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -10.16 15.24 0) (length 5.08)
        (name "VBUS"
          (effects (font (size 1.016 1.016)))
        )
        (number "B4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -10.16 15.24 0) (length 5.08)
        (name "VBUS"
          (effects (font (size 1.016 1.016)))
        )
        (number "B9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -10.16 10.16 0) (length 5.08)
        (name "CC1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -10.16 7.62 0) (length 5.08)
        (name "CC2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -10.16 5.08 0) (length 5.08)
        (name "DP1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -10.16 2.54 0) (length 5.08)
        (name "DP2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -10.16 0.0 0) (length 5.08)
        (name "DN1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -10.16 -2.54 0) (length 5.08)
        (name "DN2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -10.16 -5.08 0) (length 5.08)
        (name "SBU1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -10.16 -7.62 0) (length 5.08)
        (name "SBU2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -10.16 -15.24 0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "A1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -10.16 -15.24 0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "A12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -10.16 -15.24 0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "B1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -10.16 -15.24 0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "B12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -10.16 -12.7 0) (length 5.08)
        (name "SHELL"
          (effects (font (size 1.016 1.016)))
        )
        (number "S1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -10.16 -12.7 0) (length 5.08)
        (name "SHELL"
          (effects (font (size 1.016 1.016)))
        )
        (number "S2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -10.16 -12.7 0) (length 5.08)
        (name "SHELL"
          (effects (font (size 1.016 1.016)))
        )
        (number "S3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -10.16 -12.7 0) (length 5.08)
        (name "SHELL"
          (effects (font (size 1.016 1.016)))
        )
        (number "S4"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)